# Weekly Fish and Water Operations Outlook

11/5/2024 – 11/11/2024

## Water Project Operational Intent for Week

Both (CVP and SWP) water projects are operating to the following D-1641 standards: 1) monthly average Delta Outflow (and Rio Vista flow) not less than 4,500 cfs in November, 2) E/I ratio no greater than 0.65, and 3) daily Chlorides at Contra Costa Intake (at Rock Slough) no greater than 250 mg/l.

## Biological Context

No ESA biological protections “controlling” water project operations have been “triggered” at this time.

## Forecasted Weather

Mostly dry conditions this week with near normal temperatures. North winds, particularly in afternoon, increase in intensity during mid-week elevating fire weather concerns.

## Tables

Table 1: Anticipated weekly operational ranges by tributary. Environmental and fish conditions are updated by respective watershed groups at varying intervals that may not coincide with the weekly range of Water Operations shown.

| Tributary/Division | Anticipated Weekly Ranges | Related Environmental and Fish Conditions |
| --- | --- | --- |
| Clear Creek | * Current Release: 200 cfs * Anticipated Weekly Range of Releases: 200 cfs. | * Fall-run Chinook Salmon actively spawning and their eggs incubating. * Spring-run Chinook Salmon eggs are incubating. * O. mykiss adults are migrating into the creek. * (Updated 10/28/2024) |
| Sacramento River | * Shasta Storage: 2.577 MAF * Current Release: 6,200 cfs * Anticipated Weekly Range of Releases: 5,000 cfs to 6,200 cfs. | * Winter-run adult spawning is complete, some winter-run fry remain in gravel * Spring-run adults have completed spawning, spring run eggs/fry remain in the gravel. * Fall-run adults are actively spawning, fall-run eggs/fry are in the gravel. * Late-fall adults are migrating upstream from the ocean and holding in the watershed. * Winter-run fry are migrating past RBDD in relatively low numbers considering that historically 72% of the run has passed through by this time. * Small numbers of late fall-run pre-smolts, late fall-run juveniles from last spring, spring-run and fall-run smolts, and O. Mykiss juveniles also passing RBDD at this time. * (Updated 11/54/2024) |
| Feather River | * Oroville Storage: 1.704 MAF * Current Release: 1,750 cfs * Anticipated Weekly Range of Releases: 1,750 cfs * Daily temperature maximum: 51 +/- 4 degrees F at Fish Hatchery | * Spring-run Chinook spawning is complete, eggs are incubating in gravel. * Fall-run Chinook salmon adults are migrating upstream and spawning. * Adult O. mykiss present and migrating upstream. * (Updated 10/28/2024) |
| American River | * Folsom Storage: 391 TAF * Current Release: 2,000 cfs * Anticipated Weekly Range of Releases: 2,000 cfs | * Fall-run Chinook salmon adults are migrating upstream and beginning to spawn. * 11 fall-run redds have been observed so far in river. * (Updated 11/4/2024) |
| Stanislaus River | * New Melones Storage: 1.796 MAF * Current Release: 500 cfs * Anticipated Range of Weekly Releases: 200 cfs to 500 cfs for Fall Pulse Flow. | * Juvenile and adult O. mykiss are present. * Adult fall-run Chinook Salmon are migrating upstream and beginning to spawn. * Redds are beginning to be observed in river. * (Updated 14/4/2024) |
| Delta | * Freeport: 8,000 to 10,000 cfs * Vernalis: 1,000 to 2,500 cfs * Delta Outflow index: 4,000 to 5,800 cfs * Combined Exports: 4,500 to 7,000 cfs * JPP: 3,500 cfs * CCF: 1,000 cfs to 3,500 cfs * Expected Daily OMR Index Values: -3,500 to -5,700 cfs * DCC Gates: Opened on 10/11. * X2 > 81 km * Tides: Transition from Spring to Neap; Full Moon on 11/15. | * Delta Smelt juveniles, sub-adults and adults are expected to be present in the Low Salinity Zone and the Sacramento Deepwater Shipping Channel. No Delta Smelt have been detected in WY2025. * No Longfin Smelt have been detected upstream of the confluence in WY2025. * (Updated 11/5/2024) |

Table 2a-b: WY 2025 relevant Fish and Environmental Criteria and Status in 2019 Reclamation LTO Action Cumulative loss for the duration of 2019 Biological Opinion began upon signature of ROD, 2/19/2020.

Table 2a: WY 2025 Salmonid Current Loss and Delta Smelt Abiotic Conditions. Additional Real-Time OMR Restrictions and Performance Objectives (4.10.5.10.2, 4.10.5.10.3) and Onset of OMR Management (4.10.5.10.1). Genetic identification of salmon is not used in calculating loss, but results are included in the Assessment as they become available.

| Species/run | Threshold | Current Status | Weekly Trend | Updated |
| --- | --- | --- | --- | --- |
| Green sturgeon | WY 2025 salvage = 74 | WY 2025 salvage = 0 (0%) | No change expected | 11/04/2024 |
| Natural winter-run Chinook Salmon | WY 2025 loss = TBD \*  (50% of 1.17% of JPE) | WY 2025 loss = 0 | No change expected | 11/04/2024 |
| Natural Steelhead | Dec 1 – Mar 31 = 707 (50% of 1,414)  Apr 1 – June 15 = 776 (50% of 1,552) | WY 2025 loss = 0  Dec 1 – Mar 31 = 0 (0%)  Apr 1 – June 15 = 0 (0%) | No change expected | 11/04/2024 |
| Sacramento River Hatchery winter-run Chinook salmon | WY 2025 loss = TBD\* (50% of 0.12% of JPE) | WY 2025 loss = 0 (0%) | No change expected | 11/04/2024 |
| Battle Creek  Hatchery winter-run Chinook salmon | WY 2025 loss = TBD \*  (50% of 0.12% of JPE) | WY 2025 loss = 0 (0%) | No change expected | 11/04/2024 |
| Proposed Action Hatchery yearling spring-run Chinook salmon surrogates | > 0.5% of each release group | WY 2025 loss = 0 (0%)\* | No change expected | 11/04/2024 |
| Delta Smelt | After Dec. 1:  Running 3-day avg. flows at Freeport >25,000 cfs  Running 3-day avg. turbidity at Freeport =>50 FNU | Freeport 3-day avg.  Flow = 8641 cfs  Turbidity = 2.84 FNU | No change expected | 11/4/2024 |
| Delta Smelt | Daily avg. Turbidity at OBI=>12 FNU | OBI Daily Average = Not relevant | Not relevant | 10/28/2024 |
| Delta Smelt | Daily avg. Temperature at CCF > 25°C for three consecutive days | CCF daily avg. Temperature = Not relevant | Not relevant | 10/28/2024 |

Table 2b. 10-Year Salmonid Cumulative Loss

| Species/run | Threshold | Current Status | Updated |
| --- | --- | --- | --- |
| Natural winter-run Chinook salmon | Loss = 8,738 | Cumulative loss =  4575.3 (52.36%) | 11/04/2024 |
| Hatchery winter-run Chinook salmon | Loss = 5,356 | Cumulative loss =  11.04 (0.21%) | 11/04/2024 |
| Natural steelhead | Loss = 6,038 (Dec 1 – Mar 31) Loss = 5,826 (Apr 1 – June 15) | Cumulative loss =  4951.27 (82%, Dec 1 – Mar 31)  2923.28 (50.2%, Apr 1 – June 15) | 11/04/2024 |

Table 3a-d: Relevant Water Year 2025 Fish Criteria and Status for Listed Fish under the SWP Long-Term Incidental Take Permit.

Table 3a: Chinook Salmon

\* No draft WR JPE for WY 2025. Final JPE letter is expected in January.

| Action | Timeframe | Current Action Status | Threshold(s) | Current Relevant Data | Weekly Trend | Last  Updated | Comments |
| --- | --- | --- | --- | --- | --- | --- | --- |
| OMR Mgmt.  triggered (8.3.2) | Jan. 1 - Jun. 30  *(when ≥ 5% of spring-run or winter- run in*  *Delta)* | Not in effect | -5% of the  Winter-run or Spring-run population in  Delta | N/A | N/A | 10/7/24 | N/A |
| Winter-run yearly loss  (8.6.1) | Nov. 1 - Jun. 30 | In effect | TBD (based on JPE)\* | N/A | N/A | 10/7/24 | N/A |
| Winter-run discrete daily loss (8.6.2) | Nov. 1 - Dec. 31 | In effect | 11/1-11/30: loss of 6/day unclipped older juv. Chinook Salmon | N/A | N/A | 11/4/24 | N/A |
| Mid and late season Winter-run daily loss threshold (8.6.3) | Jan 1 – May 31 | Not in effect | TBD (based on JPE)\* | N/A | N/A | 10/7/24 | N/A |
| Spring-run surrogate protection  (8.6.4) | Feb. 1 - Jun. 30 | Not in effect | TBD (based on the number of fish released) | N/A | N/A | 10/7/24 | N/A |

Table 3b: Delta Smelt

| Action | Timeframe | Current Action Status | Threshold(s) | Current Relevant Data | Weekly Trend | Last Updated | Comments |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Integrated Early Winter Pulse Protection ('First Flush') (8.3.1) | Dec. 1 - Jan. 31 | Not active | - three-day Freeport daily flow running avg>= 25,000 AND  [three-day Freeport turbidity running avg >=50 NTU OR Smelt Monitoring Team recommendation] | FPT flow: 8641 cfs  FPT turbidity: 2.84 FNU | No change expected | 11/4/24 | Data from 11/3/24 |
| Turbidity Bridge Avoidance (8.5.1) | Dec. 15 -  Apr. 1 | Not active | Occurs after the Integrated Early Winter Pulse protection or February 1 (whichever comes first) until April 1  -avg. OBI turbidity>12 FNU | OBI Turbidity: Not relevant | Not relevant |  |  |
| Larval and/Juvenile Delta smelt Protection (8.5.2) | ongoing | Not active | - If 5-day cum. salvage of juv.DS >= 1[average 3-yrFMWT index + 1], then –5000 OMR  - If DS in SLS/20mm or 3-d temp at Jersey Point >= 12C, and SLS/20mm Secchi for 12 south delta stations <= 1m, then –3500 OMR | Current 5-day salvage = Not relevant  3-day SJJ temp = Not relevant  Secchi = Not relevant | Not relevant |  | N/A |

Table 3c: Longfin Smelt

| Action | Timeframe | Current Action Status | Threshold(s) | Current Relevant Data | Weekly Trend | Last Updated | Comments |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Early Adult Protection (8.3.3) | Dec. 1 - Feb. 28 | Not Active | -Cum. salvage > [most recent FMWT/10] =XX fish (Sept.-Dec. Index) OR  -Smelt Monitoring Team determines high likelihood of LFS movement into high-risk areas | Cum salvage total = 0 | No change expected | 11/04/24 |  |
| OMR Mgt. for Adults (8.4.1) | Dec. 1 -Feb. 28 | Not Active | -Smelt Monitoring Team recommendation | N/A | N/A |  | N/A |
| Larval and Juvenile Longfin Smelt Entrainment Protection (8.4.2) | Jan 1 – Jun 30 | Not Active | -LFS larvae or juveniles in >=4 SLS or 20 mm stations in central and south Delta, OR  -LFS catch/tow >5 larvae or juveniles in >=2stations |  |  |  |  |
| High Flow OMR Off-Ramp for Longfin Smelt (8.4.3) | Based on the status of 8.3.3, 8.4.1, & 8.4.2 | Not Active | -Sac. R. at Rio Vista>55,000, OR  SJR at Vernalis >8,000 | Rio Vista = 3,500 – 5,500 cfs  SJ = 1,000 to 2,500 cfs | N/A | 11/4/24 | N/A |

Table 3d: OMR

| Action | Timeframe | Current Action Status | Threshold(s) | Current Relevant Data | Weekly Trend | Last Updated | Comments |
| --- | --- | --- | --- | --- | --- | --- | --- |
| OMR Storm Flexibility (8.7) | Jan 1 – Jun 30 | Not in Effect | -Delta is in excess  -QWEST is > 0  -Measurable amount of precipitation has occurred  -None of COA’s are controlling operations (8.3.1, 8.3.3, 8.4.1, 8.4.2, 8.5.1, 8.5.2, 8.6.1, 8.6.2, 8.6.3, 8.6.4)  -Cumulative salvage at CVP and SWP of yearling CNFH LFR Chinook salmon (as yearling CHNSR surrogates) is < 0.5% with any of the release groups  -Risk Assessments conducted by the SaMT/SMT determines no changes in spawning, rearing, foraging, sheltering, or migration behavior as a result of OMR Flex operations beyond those are likely to occur. | N/A | N/A | 10/14/24 | Based on storm conditions |
| OMR  Mgmt.  Offramp  (8.8) | Jun. 1 – Jun. 30 | Not in effect | ->95% of the Winter-run and Spring run populations have migrated past Chipps Island AND  -Current daily average water temperature at Mossdale and Prisoners Point. | N/A | N/A | 10/14/24 | N/A |

Table 4: Fish monitoring gear efficiency and disruptions. Status Categories: [1] Active (ongoing sampling), [2] Partial Interruption (some sampling interruptions), [3] Interrupted (sampling fully suspended), [4] Not Active (sampling not scheduled)

| Monitoring survey | Region | Notes (as of 11/5/2024) | Status |
| --- | --- | --- | --- |
| SWP regular counts, CWT reading | Delta | Active | 1 |
| SWP larval sampling | Delta | Not Active | 4 |
| CVP regular counts, CWT reading | Delta | Active | 1 |
| CVP larval sampling | Delta | Not Active | 4 |
| Smelt Larval Survey | Delta | Not Active | 4 |
| LEPS | Delta | Not Active | 4 |
| 20mm Survey | Delta | Not Active | 4 |
| Fall Mid-water Trawl | Delta | Active | 1 |
| Summer Townet Survey | Delta | Not Active | 4 |
| Bay Study | Delta | Active | 1 |
| DJFMP- Chipps and Sacramento Trawls | Delta | Active | 1 |
| DJFMP- Seines | Delta | Active | 1 |
| EDSM | Delta | Active | 1 |
| EMP | Delta | Active | 1 |
| Mossdale | Delta | Active | 1 |
| USGS Flow monitoring | Delta | Active | 1 |
| Red Bluff Diversion Dam Rotary Screw Trap (RST) | Sacramento River | Active | 1 |
| Knights Landing RST | Sacramento River | Active | 1 |
| Tisdale RST | Sacramento River | Active | 1 |
| GCID RST | Sacramento River | Not Active | 4 |
| Yuba River (Hallwood) RST | Yuba River | Active | 1 |
| Butte Creek Carcass Surveys | Butte Creek | Active | 1 |
| Butte Creek RST | Butte Creek | Active | 1 |
| Redd dewatering and stranding surveys | Sacramento River | Active | 1 |
| Sacramento Carcass and Redd Surveys | Sacramento River | Active | 1 |
| Lower Sacramento RST | Sacramento River | Active | 1 |
| Feather River (upper DWR) RST | Sacramento River | Not Active | 4 |
| Feather River (lower CDFW) RST | Sacramento River | Not Active | 4 |
| Feather River Carcass Survey | Sacramento River | Active | 1 |
| SJRRP CDFW Field Monitoring | San Joaquin River | Active | 1 |
| SJRRP USFWS and USBR Field Monitoring | San Joaquin River | Active | 1 |
| Stanislaus Fish Weir | San Joaquin River | Active | 1 |
| Stanislaus River Carcass Survey | San Joaquin River | Active | 1 |
| American River Carcass Survey | Sacramento River | Active | 1 |

Preference (i.e., a y-intercept of 0.5)